**Straight Nylon grab bar, anti-bacterial NylonClean, 500mm**

Bright white HR anti-bacterial Nylon

Ø 32mm

Reference: **50505N**

Specification description

Straight grab bar for people with reduced mobility.

Straight grab bar made from bright white HR Nylon

For use as a handrail and grab bar for WCs, showers or baths.

NylonClean anti-bacterial treatment: optimal protection against bacterial development and mould.

Suitable for intensive use in public places or the healthcare sector.

High strength polyamide (Nylon): with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning.

Anti-UV treatment: prevents yellowing.

Warm to the touch.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings, secured to wall by a 6-hole cover plate, Ø 73mm.

Supplied with stainless steel screws for concrete walls.

Ø 32mm tube, 500mm centres.

Tested to over 200kg. Maximum recommended user weight: 135kg.

30-year warranty.

CE marked.