**Corner grab bar, white anti-bacterial Nylon**

Bright white NylonClean anti-bacterial HR Nylon,

Ø 32mm, for hung shower seats

Reference: **5121N**

Specification description

Two-wall corner shower grab bar Ø 32mm, for people with reduced mobility.

Can be used as a support rail to support the user in an upright position.

Helps and secures movement in the shower, or to get into or out of the bath.

For WCs with a recessed cistern or direct flush, helps transfer from a wheelchair to the toilet.

NylonClean anti-bacterial treatment: optimal protection against bacterial development.

Can support a removable shower seat (order separately).

Suitable for intensive use in public places or the healthcare sector.

High strength polyamide (Nylon): with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning. Anti-UV treatment.

Warm to the touch.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Fixings concealed by a 6-hole cover plate, Ø 73mm.

Supplied with stainless steel screws for concrete walls.

Dimensions: 750 x 750mm.

Tested to over 200kg. Maximum recommended user weight 135kg.

Angled grab bar with 30-year warranty. CE marked.