**Wall-mounted mechanical sink mixer**

Wall-mounted mixer with swivelling spout L. 200mm

With offset standard connectors

Reference: **5445T2S**

Specification description

Wall-mounted mechanical sink mixer with swivelling, Ø 22mm tubular under-spout L. 200mm with star-shaped, brass flow straightener.

 Spout with smooth interior (reduced bacterial development).

 Flow rate 45 lpm at 3 bar.

Chrome-plated metal control knobs with ceramic valve heads.

Supplied with offset standard connectors, M1/2" M3/4".

 30-year warranty.