**TEMPOMATIC MIX 3 electronic mixer**

Integrated batteries, Ø 15mm stopcocks

Standard control, Integrated electronics

Reference: **49200615**

Specification description

Deck-mounted electronic basin mixer:

Battery-operated with integrated 223 CR-P2 6V Lithium batteries.

Reduced stagnation solenoid valve and electronic unit integrated into the body of the mixer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Chrome-plated solid brass body.

Cap fixed in place by two concealed screws, with pictogram to identify sensor easily.

PEX flexibles Ø 15mm for compression fittings with stopcocks, filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Side temperature control with adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.