**SPORTING time flow shower kit**

Time flow

Exposed, TONIC JET head, valve

Reference: **714000**

Specification description

Time flow shower kit for exposed installation:

SPORTING time flow valve M½" for top inlet supply with mixed water.

For wall-mounted, exposed installation.

Reinforced shower column Ø 16mm and collar.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Tamperproof, scale-resistant fixed showerhead with automatic flow rate regulation.

De-pressurising push-button.

Fixings with stainless steel screws supplied.

Chrome-plated solid brass body.

Integrated non-return valve and filter.

Suitable for people with reduced mobility.

30-year warranty.