**Straight stainless steel grab bar, satin, Ø 32mm, 500mm**

UltraSatin polished satin stainless steel

Ø 32mm

Reference: **50505S**

Specification description

Straight grab bar for people with reduced mobility.

Tube Ø 32mm, 500mm centres.

For use as a handrail and grab or support bar for WCs, showers or baths.

Can be used to hang a shower seat on (order separately).

Straight grab bar made from bacteriostatic 304 stainless steel tube.

Stainless steel with UltraSatin satin finish, non-porous uniform surface for easy maintenance and hygiene.

Plate welded to the tube by invisible bead weld (process exclusive to ArN-Securit).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings secured by a 3-hole plate, 304 stainless steel, Ø 72mm.

Fixing plates and cover plates made from 304 stainless steel.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 135kg.

30-year warranty. CE marked.