**MINERALCAST wash trough**

MINERALCAST - 3 services - L. 1400mm

With Ø 35mm central tap hole

Reference: **453140**

Specification description

Wall-mounted wash trough, 3 services.

MINERALCAST: composite material consisting of natural minerals and polyester resin.

Ideal for use in public and commercial places, especially schools.

Uniform, non-porous surface is easy to clean.

One-piece cast wash trough, seam-free, for easy maintenance and better hygiene.

Warm to the touch.

With incline to prevent water pooling.

With Ø 35mm central tap hole.

Supplied with three 1¼" wastes. Without overflow.

Supplied with fixing elements.

White, RAL 9016.

CE marked. Complies with European standard EN 14296.

Weight: 63kg.

30-year warranty.