**Mechanical sink or trough mixer**

Single hole, single control tall mixer with ceramic cartridge

Mixer with swivelling, removable st. steel spout

Reference: **2870T3**

Specification description

Deck-mounted mechanical sink mixer.

Single hole, single control mixer with high, swivelling spout H. 320mm.

Mixer supplied with 2 removable stainless steel spouts.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduced bacterial development).

Thermal shocks are possible without removing the control lever or shutting off the cold water.

Flow rate limited to 9 lpm at 3 bar.

Touch-free control via the Hygiene lever L. 185mm.

Body and base in chrome plated brass.

PEX flexibles F3/8".

Fixing reinforced by 2 stainless steel rods.

Mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.