**DUPLO RP wall-mounted multiple washbasin**

Polished satin 304 stainless steel - L. 1200mm - With splashback

With central tap hole, Ø 35mm

Reference: **121390**

Specification description

Wash trough for wall-mounting, for 2 services, 1,200x500mm.

With a splashbaack to protect the wall from splashing and improve hygiene.

Basin internal diameter: 310mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm.

Rounded edges prevent injury.

With Ø 35mm central tap hole.

Supplied with x2 1¼" wastes.

Without overflow.

Supplied with brackets and fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 15kg.

30-year warranty.

[Formerly ref: 0211390008]