**BCN P floor-standing stainless steel pan**

Polished satin 304 stainless steel

Reference: **110100**

Specification description

Floor-standing WC pan, 360 x 400 x 580mm.

Elegant and simple design.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm.

One-piece pressed WC bowl, seam-free for easy maintenance and better hygiene.

WC bowl surface is polished with rounded edges for easy cleaning.

Concealed perimetral flushing rim.

Horizontal water inlet: Ø 55mm.

Horizontal or vertical waste outlet: Ø 100mm. Supplied with PVC pipe.

Water saving: works with 4L or more of water.

Pre-drilled holes for fixing the toilet seat. Supplied with stainless steel blanking caps when installed without toilet seat lid.

Quick and easy to install: 2 access panels with theft prevention TORX security screws.

CE marked. Complies with European standard EN 997 for 4L flush.

Weight: 12kg.

30-year warranty.

[Formerly ref: 0110100001]