**Single L stall urinal**

Polished satin 304 stainless steel - L. 600mm - Floor-recessed

Reference: **130200**

Specification description

Trough urinal for recessing in the floor, 600 x 1020 x 300mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rear water inlet.

Supplied with 1 stainless steel rinser and 1 flexible hose.

Water saving: optimal rinsing with 0.1 L/sec. per service i.e. 0.3L per use.

Central drainage.

Waste outlet 1½". Supplied with waste and integrated trap (ref. 785000).

Weight: 16.8kg.

[Formerly ref: 0310200001]