**TEK TC washbasin**

Polished satin 304 stainless steel - Wall-mounted with concealed waste

With integrated tap

Reference: **160340**

Specification description

Wall-mounted washbasin, cross wall installation for service ducts.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Vandal-resistant: shrouded basin, concealed waste outlet.

200mm threaded rod can be cut to size (other lengths available on request.

Supplied with 1 time flow tap: stainless steel tamperproof push-button and anti-blocking, 7 seconds time flow.

Recessed horizontal waste outlet Ø 32mm.

Flat, perforated waste, without screws: easy to clean and vandal-resistant.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 9kg.

[Formerly ref: 3416340000]