**S21 S TC wall-hung WC pan**

Polished satin 304 stainless steel - vandal-resistant

Reference: **160310**

Specification description

Wall-hung WC pan with through-the-wall installation for service ducts.

Elegant and simple design.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm

One-piece pressed WC bowl, seam-free for easy maintenance and better hygiene.

WC bowl surface is polished with rounded edges for easy cleaning.

Concealed perimetral flushing rim.

Horizontal water inlet: Ø 55mm

Horizontal waste outlet: Ø 100mm

Water saving: works with 4L or more of water.

200mm threaded rod can be cut to size (other lengths are available on request).

 Shrouded WC pan.

CE marked. Complies with European standard EN 997 for 4L flush.

Weight: 11kg.

[Formerly ref: 0116320001]