**Floor-standing janitorial unit**

Polished satin 304 stainless steel

With tap hole Ø 35mm on right side

Reference: **180140**

Specification description

Floor-standing janitorial unit.

Bacteriostatic 304 stainless steel. Polished satin finish.

Stainless steel thickness: 1.0mm.

Smooth surface for easy cleaning.

Adjustable feet height up to 25mm.

Easy to maintain: front access panel.

With tap hole Ø 35mm on right side.

Supplied with 1¼" waste for washbasin and 1½" for disposal sink. Without overflow.

Hinged stainless steel bucket grid.

CE marked. Complies with norm EN 14688.

Weight: 22kg.

30-year warranty.

[Formerly ref: 0710140000]