**Wall-mounted SXS electronic hand washbasin**

Polished satin 304 stainless steel - electronic control - with upstand

With tap and soap dispenser

Reference: **184320**

Specification description

Wall-mounted hand washbasin with electronic control.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

With splashback.

Supplied with battery-operated electronic mixer with integrated batteries and solenoid valve, and chrome-plated brass soap or hydroalcoholic gel dispenser.

1¼" waste included. Without overflow.

Water savings: flow rate pre-set at 3 lpm.

Maximum hygiene: no manual contact with tap, reduced stagnation solenoid valve, duty flush prevents bacterial development.

Supplied with fixings.

CE marked. Complies with European standard EN 14688.

Weight: 4.1kg.

30-year warranty.