**Rectangular stainless steel mirror, H. 1000mm**

Unbreakable mirror

"Mirror" polished 304 stainless steel

Reference: **3459**

Specification description

Wall-mounted rectangular mirror made from "mirror" polished bacteriostatic 304 stainless steel.

For combined installation: height enables use from standing or sitting positions, or from a wheelchair.

Reinforced by a concealed, solid, 10mm thick PVC plate.

5 fixing points. Concealed fixings.

For installation on a flat surface.

Unbreakable mirror.

Dimensions: 10 x 595 x 980mm.

30-year warranty.