**T-shaped Nylon grab bar with sliding vertical bar, white**

Bright white NylonClean anti-bacterial HR Nylon

Ø 32mm

Reference: **5441N**

Specification description

T-shaped grab bar with sliding vertical bar Ø 32mm, for people with reduced mobility.

Use as a grab bar and to support the user in an upright position.

Helps and secures entry and movement in the shower.

Use as a shower rail by adding a shower head holder and/or soap dish.

Anti-bacterial NylonClean treatment: increased protection against bacterial development.

Upright position can be adjusted during installation: can be moved to the left or the right in order to adapt the space (positioning of shower, depth of shower seat...).

Suitable for intensive use in commercial environment or healthcare.

High-strength polyamide (Nylon): with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning. Anti-UV treatment.

Warm to the touch.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings, secured to wall by a 6-hole plate, Ø 73mm.

Supplied with stainless steel screws for concrete walls.

Dimensions: 1,150 x 500mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

 30-year warranty. CE marked.