**TEMPOFLUX control plate for urinals**

Time flow valve 7 sec with soft-touch operation - For urinals

Satin stainless steel plate

Reference: **778707**

Specification description

Control plate and time flow valve TEMPOFLUX F½", kit 2/2:

Satin finish stainless steel wall plate 145 x 145mm.

Chrome-plated metal button.

Soft-touch operation.

Time flow pre-set at ~7 seconds.

Flow rate pre-set at 0.15 L/sec. at 3 bar, can be adjusted up to 0.3 L/sec.

Compatible with sea water, rain water and grey water.

Complies with European standard EN 12541 (class II acoustic level).

Install in waterproof housing with waterproof collar, filter and stopcock.

Suitable for people with reduced mobility.

30-year warranty.

Order with frame system references 543006 for urinals Ø 35mm, 543006D for urinals with flexible ½" or with 778BOX recessed housing.