**TEMPOFLUX 2 control plate for WCs**

Soft-touch operation time flow valve, 3L/6L dual flush

For walls 10-35mm - Chrome-plated metal plate

Reference: **578222**

Specification description

Control plate for TEMPOFLUX 2 time flow direct flush, kit 2/2:

Flush system without cistern, directly connected to pipework.

Ø 195mm chrome-plated metal wall plate.

Concealed mechanical fixing of the wall plate.

3L/6L dual flush can be adjusted to 2L/4L.

Soft-touch operation.

For walls 10 - 35mm.

Complies with European standard EN 12541 class II.

30-year warranty.

Order with frame system references 578305DE, 578300DE, 578405DE or 578400DE.