**TEMPOFLUX 3 control plate for WCs**

Soft-touch operation time flow control, AB, recessed

6L single flush plate - chrome-plated metial

Reference: **763041**

Specification description

Control plate and recessed time flow direct flush valve TEMPOFLUX 3, kit 2/2:

Flush system without cistern: directly connected to pipework.

Chrome-plated metal plate 170x 170mm.

Mechanical fixing of the plates.

TEMPOFLUX 3 F¾" valve compatible with sea water, rain water and grey water.

Soft-touch operation.

AB anti-blocking system: flush only takes place once the push-button is released.

6L single flush. Round design.

Complies with European standard EN 12541 (class II acoustic level).

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Suitable for rimless WC pans without flow rate regulation and suitable for people with reduced mobility.

30-year warranty.

Order with frame system reference 564065DE or 564060DE, or with 763BOX recessed housing.