**MONOBLOCO S21 WC pan with cistern**

Matte black 304 stainless steel

Reference: **110390BK**

Specification description

Floor-standing WC pan with dual flush cistern 3L/6L.

Bacteriostatic 304 stainless steel. Stainless steel thickness: 1.5mm.

Matte black Teflon® finish.

WC bowl surface is polished with rounded edges for easy cleaning.

Concealed perimetral flushing rim. Water supply can be recessed from below or exposed from the side (right/left).

Recessed horizontal or vertical waste outlet. Supplied with PVC pipe.

Pre-drilled holes for fixing the toilet seat. Supplied with stainless steel blanking caps when installed without toilet seat lid.

Quick to install: 2 access panels with theft prevention TORX security screws.

CE marked. Complies with European standard EN 997 for 4L flush.

Weight: 21kg.

30-year warranty.