**TEMPOFLUX 3 AB flush kit**

Anti-blocking direct flush WC kit

Cross wall 200mm with tube

Reference: **763266**

Specification description

Flush system without cistern: directly connected to pipework.

For walls ≤ 200mm.

Soft-touch operation.

AB anti-blocking system: flush only takes place once the push-button is released.

Time flow ~7 seconds.

Vacuum breaker.

Stopcock and volume/flow rate adjustment, activation unit and cartridge are all integrated and accessible via the service duct.

Chrome-plated metal push-button.

Shock-resistant mechanism.

In-line inlet M¾".

Complies with European standard EN 12541 (class II acoustic level).

Cut-to-size threaded rod.

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

With Ø 32mm PVC flush tube.

Compatible with rain water.

Suitable for rimless WC pans without flow rate regulation and suitable for people with reduced mobility.

30-year warranty.