**Recessing housing for thermostatic shower mixers**

Sequential mixer, kit 1/2

For recessing, with angled outlet, waterproof

Reference: **H96CBOX**

Specification description

Waterproof recessing housing for sequential thermostatic shower mixer, kit 1/2:

- Collar with waterproof seal.

- Hydraulic connection from the outside and maintenance from the front.

- Water supply connects from the top.

- Adjusts to all types of installations (rails, solid walls, panels).

- Compatible with wall finishes 10 - 120mm (while maintaining the minimum recessing depth of 80mm).

- Suitable for standard or "pipe-in-pipe" supply.

- Stopcocks and flow rate adjustment, filters, non-return valves and cartridge are all integrated and accessible from the front.

- Sequential thermostatic shower mixer.

- Supplied in 2 kits: secure system flush without sensitive elements.

30-year warranty.

Order with the control plate reference H9633.