**Recessing housing for mechanical shower mixers**

Mechanical mixer, kit 1/2

Recessed with angled outlet, waterproof

Reference: **254CBOX**

Specification description

Waterproof recessing housing for mechanical shower mixers, kit 1/2.

- Collar with waterproof seal.

- Hydraulic connection from the outside and maintenance from the front.

- Top inlets.

- Adjusts to all types of installations (rails, solid walls, panels).

- Compatible with wall finishes 10 - 120mm (while maintaining the minimum recessing depth of 93mm).

- Suitable for standard or "pipe-in-pipe" supply.

- Stopcocks and flow rate adjustment, filters, non-return valves and cartridge are all integrated and accessible from the front.

- Mechanical shower mixer.

- Supplied in 2 kits: secure system flush without sensitive elements.

30-year warranty.

Order with a control plate reference 2551 or 2551EP.