**Recessed mechanical shower mixer**

Mechanical mixer in a waterproof housing, kit 2/2

Shower head not included

Reference: **2541**

Specification description

Mechanical shower mixer which can be recessed; kit 2/2.

Single control mixer with Ø 40mm ceramic cartridge.

Pre-set maximum temperature limiter.

Thermal shocks are easy to undertake without removing the control lever or shutting off the cold water.

Flow rate regulated at 9 lpm (mixer only), 6 lpm at 3 bar with shower head.

Solid control lever.

Order a shower head to complete.

Bright polished stainless steel cover plate 166 x 166mm.

Mechanical shower mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.

Order with a waterproof recessing housing ref. 254BOX.