**Be-Line® WC pack with backrest**

DOC M pack

Metallised anthracite powder-coated aluminium

Reference: **511809MC**

Specification description

DOC M Be-Line® WC pack with 1 backrest, depth 150mm.

1 drop-down support rail, length 850mm.

4 grab bars, length 600mm.

Aluminium tube.

Metallised anthracite powder-coated finish (LRV 14) provides a good visual contrast with the wall.

Tested to over 200kg.

Maximum recommended user weight 135kg.

30-year warranty.

CE marked.

DOC M compliant.