**TEMPOMATIC 4 waterproof housing for showers**

Mains supply, kit 1/2

Recessed, waterproof

Reference: **443SBOX**

Specification description

TEMPOMATIC 4 waterproof housing for showers kit 1/2:

Collar with waterproof seal.

Hydraulic connection to the outside and maintenance from the front.

Adjusts to all types of installation (rails, solid walls, panels).

Compatible with wall finishes 10 - 120mm (while maintaining the minimum recessing depth of 93mm).

Integrated stopcocks, flow regulator, filter, non-return valve and cartridge, accessible from the front.

Supplied in 2 kits: to allow secure system flush without sensitive elements.

30-year warranty.

Order with control plate only, reference 443228 or complete shower kit, reference 443229.