**Waterproof housing for TEMPOSOFT 2 showers**

Time flow, kit 1/2

Recessed, waterproof

Reference: **748BOX**

Specification description

Recessed waterproof housing for TEMPOSOFT 2 showers kit 1/2 :

Collar with waterproof seal.

Hydraulic connection from the outside and maintenance from the front.

Adjusts to all types of installations (rails, solid walls, panels).

Compatible with wall finishes 10 - 120mm (while maintaining the minimum recessing depth of 93mm).

Stopcocks and flow rate adjustment, filters, non-return valves and cartridge are all integrated and accessible from the front.

Supplied in 2 kits: secure system flush without sensitive elements.

30-year warranty.

Order with control plate reference 748218 or complete shower kit 748219.