**Be-Line® recessed shower pack**

DOC M pack

Metallised anthracite powder-coated aluminium

Reference: **511MREC1**

Specification description

Metallised anthracite powder-coated aluminium DOC M recessed shower pack. 19 items:

• 2 Drop-down support rails, length 850mm.

• 3 Grab bars, with ergonomic flat front face, length 600mm.

• 3 Grab bars, with ergonomic flat front face, length 450mm.

• 1 Lift-up shower seat.

• 1 Backrest, depth 150mm.

• 1 aluminium finish coat hook.

• 1 SECURITHERM single lever sequential thermostatic recessed shower mixer with angled outlet.

• 1 Chrome-plated TONIC JET shower head, tamperproof and scale-resistant, with automatic flow rate regulator set at 6 lpm.

• 1 Recessed diverter valve.

• 1 Multi-mode shower kit with 1 single jet shower head, 1 sliding soap dish for riser rails, 1 sliding shower head holder and 1 flexible shower hose.

• 1 Grab bar for use as shower riser rail, length 600mm.

• 1 Shower hose retaining collar: retains shower hose correctly.

30-year warranty.

CE marked.