**TEMPOMATIC Connect control plate for WCs**

Recessed dual control electronic battery operated valve - For WCs

Satin stainless steel control plate

Reference: **465006**

Specification description

TEMPOMATIC Connect recessed electronic valve for direct flush, kit 2/2:

Flush system without cistern: directly connected to pipework.

Battery-operated with CR123 6V Lithium batteries.

Satin finish stainless steel wall plate 186 x 186mm.

Mechanical fixing of the control plates.

TEMPOMATIC F¾" flush valve is compatible with sea water, rain water and grey water.

Telemetric presence detection range.

Detection delay is 10 seconds.

Contactless activation (by passing the hand in front of sensor at a distance of 4cm).

Flush after each user. If the user leaves the toilet without flushing, an automatic flush is activated to ensure optimum bathroom hygiene.

"Intelligent" automatic rinsing: flush volume adapts according to use - 3L "short" usage, 6L "long" usage - (can be adjusted).

Hygienic duty flush every 24 hours (can be adjusted to 12 hours or OFF) after the last use.

Bluetooth® technology connects to the DELABIE Connect app or presence detection distance can be automatically adjusted via a concealed button.

Supply diameter: minimum Ø 20mm interior at all points (including connectors).

Base flow rate: 1L/sec at 1 bar dynamic pressure.

Suitable for rimless WC pans and suitable for people with reduced mobility.

30-year warranty.

Order with frame system references 564060 or 564065, or with recessed housing 464PBOX.