**TEMPOSTOP 3 AB time flow basin tap**

Length 110 mm

Wall-mounted, 1/2"

Reference: **703300AB**

Specification description

Wall-mounted push-button basin tap:

Time flow ~7 seconds.

Pre-set flow rate 3 lpm at 3 bar, adjustable from 1.4 to 6 lpm.

Scale-resistant tamperproof flow straightener.

Chrome-plated brass body M½".

AB anti-blocking system: water only flows when push-button is released.

30-year warranty.