**Straight stainless steel grab bar, straight Ø 32mm, 400mm**

UltraPolish bright polished stainless steel

Ø 32mm

Reference: **50504P2**

Specification description

Straight grab bar for people with reduced mobility.

Tube Ø 32mm, 400mm centres.

For use as a handrail and grab bar for WCs, showers or bath tubs.

Straight grab bar made from bacteriostatic 304 stainless steel.

Stainless steel with UltraPolish bright polished finish, non-porous uniform surface for easy maintenance and hygiene.

Plate welded to the tube by invisible bead weld (process exclusive to ArN-Securit).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Fixings concealed by a 3-hole cover plate, 304 stainless steel, Ø 72mm.

Fixing plates and cover plates in 304 stainless steel.

Supplied with stainless steel screws for concrete walls.

Tested to over 250kg. Maximum recommended user weight: 170kg.

30-year warranty.

CE marked.