**White anti-bacterial Nylon drop-down rail, L. 650mm**

Bright white NylonClean anti-bacterial HR Nylon

Ø 32mm

Reference: **5160N**

Specification description

Drop-down grab bar Ø 32mm, for people with reduced mobility.

Support rail for WCs or showers.

Allows side access in the raised position.

In the lowered position use as a grab bar, for standing up and assisting movement.

Retained in upright position. Slowed down descent.

Drop-down grab bar made from bright white HR Nylon.

Suitable for intensive use in public places or the healthcare sector.

NylonClean anti-bacterial treatment: optimal protection against bacterial and mould development.

High-strength polyamide (Nylon) and polymer: with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning.

Anti-UV treatment: prevents yellowing.

Warm to the touch.

Fixings concealed by a 4mm thick 304 stainless steel cover plate.

Supplied with stainless steel screws for concrete walls.

Dimensions: 650 x 230 x 105mm.

Tested to over 200kg. Maximum recommended user weight 135kg.

30-year warranty.

CE marked.