**White anti-bacterial Nylon drop-down rail, L. 650mm, with leg**

Bright white NylonClean anti-bacterial HR Nylon

Ø 32mm

Reference: **5162N**

Specification description

Drop-down grab bar Ø 32mm with leg, for people with reduced mobility.

Drop-down grab bar for WCs or showers.

Allows side access in the raised position.

In the lowered position use as a grab bar, as a support for standing up and for assisting movement.

Retained in upright position. Slowed descent.

Drop-down grab bar made from bright white HR Nylon.

NylonClean anti-bacterial treatment: optimal protection against bacterial and mould development.

Model with automatic folding leg. To be used as reinforcement when the wall fixing alone is insufficient.

Leg height can be adjusted from 760 – 780mm.

Suitable for intensive use in public places or the healthcare sector.

High-strength polyamide (Nylon) and polymer: with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning.

Anti-UV treatment: prevents yellowing.

Warm to the touch.

Fixings concealed by a 4mm thick 304 stainless steel cover plate.

Supplied with stainless steel screws for concrete walls.

Dimensions: 650 x 800 x 105mm.

Tested to over 200kg. Maximum recommended user weight 135kg.

30-year warranty.

CE marked.