**Lift-up Comfort shower seat with backrest and leg**

Wall-mounted lift-up shower seat

White powder-coated stainless steel structure

Reference: **510436N**

Specification description

HR Comfort lift-up shower seat with leg.

Wall-mounted lift-up shower and backrest for fixed installation.

Wall-mounted shower seat for disabled people and for people with reduced mobility.

Large model.

Anti-bacterial treatment on seat and backrest: optimal protection against bacterial development and mould.

Retained in upright position. Slowed down descent.

Suitable for intensive use in public places or the healthcare sector.

Removable solid seat and backrest made from high strength polymer.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products (Betadine®) and cleaning.

Anti-UV treatment.

Warm to the touch.

Bacteriostatic 304 stainless steel structure Ø 32mm.

White powder-coated finish.

Reinforced by a folding, articulated leg made from 304 stainless steel tube Ø 25mm.

Concealed fixings secured to wall by a 304 stainless steel plate, 4mm thick.

Supplied with stainless steel screws for concrete walls.

Dimensions: 506 x 420 x 1,000mm.

Folded dimensions: 165 x 620mm.

Tested to over 250kg. Maximum recommended user weight: 170kg.

Lift-up shower seat and backrest with 30-year warranty. CE marked.