

Wall-mounted toilet brush set
Model with anti-theft lock for fixing
Bright polished 304 stainless steel

Reference: 4048P


Specification description

Wall-mounted toilet brush set. 

Wall-mounted robust model with toilet brush and anti-theft lock for fixing. 

Bacteriostatic bright polished 304 stainless steel. 

Easy to clean: plastic bowl can be removed from above. 

Plastic bowl with reservoir: avoids toilet brush sitting in residual water and reduces the risk of splashing when next used. 

Stainless steel body 1mm thick. 

Dimensions: Ø 90mm x 330mm.

30-year warranty.
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