**Wall-mounted toilet brush set**

Model with anti-theft lock for fixing

White powder-coated 304 stainless steel

Reference: **4048EW**

Specification description

Wall-mounted toilet brush set.

Robust model with toilet brush and anti-theft lock for fixing.

Bacteriostatic white powder-coated 304 stainless steel.

Easy to clean: plastic bowl can be removed from above.

Plastic bowl with reservoir: avoids toilet brush sitting in residual water and reduces the risk of splashing when next used.

Stainless steel body 1mm thick.

Dimensions: Ø 90mm x 330mm.

30-year warranty.