**Mechanical basin mixer**

Single hole mechanical mixer H. 85mm, L. 135mm

Mixer with Hygiene lever, BEL

Reference: **2520L**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mechanical mixer H. 85mm L. 135mm with BIOSAFE hygienic outlet.

Ø 40mm classic ceramic cartridge with pre-set maximum temperature limiter.

Flow rate limited to 5 lpm at 3 bar.

Hygiene control lever L. 150mm.

With ergonomic pop-up waste 1 1/4" made from stainless steel.

PEX flexibles F3/8".

Fixing reinforced via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Suitable for people with reduced mobility.

Mixer with 30-year warranty.