**Mechanical basin mixer**

Single hole mechanical mixer H. 60mm, L. 100mm

Mixer with Hygiene lever

Reference: **2220L**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mechanical mixer H. 60mm L. 100mm with hygienic flow straightener.

Ø 35mm classic ceramic cartridge with pre-set maximum temperature limiter.

Flow rate regulated to 5 lpm at 3 bar.

Hygiene control lever L. 150mm.

With 1 1/4" pop-up waste in polypropylene.

PEX flexibles F3/8".

Reinforced fixing.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole suitable for people with reduced mobility.

Mixer with 30-year warranty.