**Mechanical basin mixer**

Single hole mechanical mixer H. 95mm L. 120mm

Hygiene lever L. 150mm

Reference: **2720L**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mixer with curved spout H. 95mm L. 120mm fitted with a hygienic BIOSAFE outlet.

Spout suitable for fitting a BIOFIL point-of-use filter.

Ø 35mm ceramic cartridge with a pre-set maximum temperature limiter.

Body and spout with smooth interior (reduced bacterial development).

Thermal shocks are easy to undertake without removing the control lever or shutting off the water supply.

Flow rate limited to 5 lpm.

Hygiene control lever L. 150mm.

Ergonomic, stainless steel pop-up waste 1 1/4".

F3/8" PEX flexibles.

Fixing reinforced via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer with 30-year warranty.

Also available with copper tails.