**Mechanical basin mixer**

Single hole mechanical mixer with swivelling spout H. 195mm L. 150mm

With pop-up waste

Reference: **2506T1**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mechanical mixer with swivelling spout H. 195mm L. 150mm fitted with a BIOSAFE hygienic outlet.

Ø 35mm ceramic cartridge with maximum temperature limiter supplied but not installed.

Spout with smooth interior.

Flow rate limited to 5 lpm at 3 bar.

Slimline control lever.

Brass pop-up waste 1 1/4".

F3/8" PEX flexibles.

Fixing reinforced by 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.