**Mechanical mixer for sinks or troughs**

Single control single hole tall mixer with ceramic cartridge

Mechanical mixer with swivelling spout H.165 L.220

Reference: **2564T2**

Specification description

Deck-mounted mechanical basin mixer.

Single control single hole mixer with swivelling spout H. 165mm L. 220mm.

Tall mixer with BIOSAFE outlet suitable for fitting a BIOFIL point-of-use filter.

Ø 35mm classic ceramic cartridge and pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduces bacterial development).

Thermal shocks are easy to undertake without removing the control lever or shutting off the cold water supply.

Flow rate regulated at 5 lpm.

Chrome-plated brass body and base.

Hygiene control lever L. 185mm requires no manual contact.

PEX flexibles F3/8".

Fixings reinforced via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.