**Mechanical sink mixer**

Wall-mounted mixer with swivelling spout L. 200, Hygiene lever L. 150

With STOP/CHECK connectors

Reference: **2519L**

Specification description

Wall-mounted mechanical sink mixer.

Wall-mounted mixer with swivelling, tubular spout L. 200mm with smooth interior (reduces bacterial development).

Auto-draining under-spout Ø 22mm with star-shaped, brass flow straightener.

 Ø 40mm standard ceramic cartridge with pre-set maximum temperature limiter.

Flow rate 26 lpm at 3 bar.

Hygiene control lever L. 150mm.

Mixer with 150mm centres supplied with offset STOP/CHECK wall connectors, M1/2" M3/4", suitable for hospitals.

Mechanical mixer idealfor healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer with 30-year warranty.