**Mechanical sink mixer**

Wall-mounted mixer with swivelling spout L. 200, Hygiene lever L. 150

With STOP/CHECK connectors

Reference: **2519L**

Specification description

Wall-mounted mechanical sink mixer with swivelling, tubular spout L. 200mm.

Auto-draining under-spout Ø 22mm with star-shaped, brass flow straightener.

Ø 40mm ceramic cartridge with pre-set maximum temperature limiter.Spout with smooth interior (reduces bacterial development).

Flow rate 26 lpm at 3 bar.

Hygiene control lever L. 150mm.

Supplied with STOP/CHECK connectors, M1/2" M3/4", ideal for hospitals.

30-year warranty.