**Shower kit with mechanical mixer**

Mechanical mixer with long lever

With offset STOP/CHECK connectors

Reference: **2539KIT**

Specification description

Shower riser rail with mechanical shower mixer.

Shower riser kit with shower mixer with Ø 40mm ceramic cartridge.

Mixer with pre-set maximum temperature limiter.

Flow rate limited to 9 lpm at 3 bar.

Chrome-plated brass body with long sculptured lever.

M1/2" shower outlet with integrated non-return valve.

Mixer with offset STOP/CHECK wall connectors M1/2" M3/4".

• Sliding shower head holder (ref. 813) on a chrome-plated riser rail (ref. 821) with soap dish and flexible hose (ref. 834T1).

• Shower hose retaining holder (ref. 830).

Mixer suitable for healthcare facilities, retirement homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

Shower riser rail with 30-year warranty.