**F3/8" PEX flexible hoses**

M10x1, L. 525mm

2 per pack

Reference: **FLEXPEX3**

Specification description

F3/8" flexible hoses M10x1 L. 525mm made from braided stainless steel with Ø 6mm PEX core to supply mixers and taps.

Withstand thermal and chlorine shocks: maximum temperature 90°C (recommended 65°C).

Maximum pressure: 10 bar.

2 per pack.