**BINOPTIC electronic tap**

Mains supply

CW 190mm, spout with smooth interior, L.135mm

Reference: **379D13**

Specification description

Cross wall electronic basin mixer:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Filters and solenoid valves M3/8".

Chrome-plated brass body.

Chrome-plated spout L.135mm for cross wall installation ≤ 190 mm.

Cable for sensor, L. 1.20mm, flexibles and mounting all pass through the same hole.

Anti-blocking security.

Spout with smooth interior and low volume of water (reduces niches where bacteria can develop).

Suitable for people with reduced mobility.

30-year warranty.