**Fixed spout with plate**

L.120mm

Cross wall 165mm

Reference: **947151**

Specification description

Spout Ø 32mm, M1/2".

L. 120mm.

For cross wall installation for walls ≤ 165mm, with anti-rotating pin.

Threaded rod can be cut-to-size.

Chrome-plated solid brass.

Scale-resistant flow straightener pre-set at 3 lpm.

30-year warranty.