**SECURITHERM shower panel**

Thermostatic mechanical dual control

Concealed inlet, fixed head and handset, alu

Reference: **792380**

Specification description

Dual control thermostatic shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Concealed inlet via flexibles M½".

SECURITHERM thermostatic mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Non-time flow 1/4-turn valves to control flow.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation set at 6 lpm at 3 bar.

Handset with removable flexible via push-fit rapid STOP connector and wall support supplied.

Concealed fixings.

Filters and non-return valves.

Suitable for people with reduced mobility.

30-year warranty.