**TEMPOMATIC electronic shower valve**

Electronic

Recessed valve

Reference: **452565**

Specification description

Recessed electronic shower valve:

TEMPOMATIC electronic valve for mixed water supply.

Recessed installation.

Power supply by electronic unit with solenoid valve ½".

230/12V transformer.

2 operation modes:

- Automatic activation via presence detection.

- Voluntary ON/OFF activation by passing hand in front of sensor ~10 cm.

Duty flush (~60 seconds every 24 hours after the last use).

Adjustable time flow from 30 to 60 seconds.

Flow rate 20 lpm.

Chrome-plated solid brass.

Electronic shower valve suitable for people with reduced mobility.

30-year warranty.

This model does not have a waterproof recessing box. The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).